; Swedish
; 
; This file provided only for translation
; English is build in language for editor
;
; format
; number=Text  control text i.e. labels, buttons
; number_h=Hint for control
; some controls have no hint message like label
; some controls have no Text message like Edit controls
; use ^m for carriage return
; use & for underline char
; use ^p for space
;
;
;

[Translations]
;Main Window
1001=X-BIOS Editor 
1002=&Open
1002_h=Open BIOS Image file
1003=&Save
1003_h=Save modified BIOS Image to file
1004=Hex editor
1004_h=Run hex editor
1005=Options
1005_h=Options
1006=Help
1007=About
1007_h=About this program
1008=Close
1008_h=Close this application

;do not forgot to place spaces for this control
1009=   General
1010= PCI Information Block
1011= BOOT screen display Infomation
1012=&Device ID
1013=&Change
1014=Sub Vendor
1015=Sub Device ID
1016=Skip DDC Monitor Detection
1017=Enable Memory Size Message
; to put Carriage return use ^m
1017_h=If On:^mWill write actual memory size ^m at boot time
1018=Enable Signon Message
1018_h=If On:^mWill write sign on message
1019=Engineering Release
1019_h=If On:^mWill write "Engineering Release" message^m(Can be safely tuned off)
1020=Shrink when save
1021= Signon messages
1022=S&ignon message
1023=Signon Color
1024_h=Sign on color^m7 - white
1025=Frames count
1026_h=Wait a number of frames^mat power on stage^m1 second = 70 frames^mDefault 280
1027=BI&OS Version message
1028=BIOS Version
1029=OEM String
1030=VESA Vendor
1031=VESA Product Name
1032=VESA Product Rev
1033=OEM Revision
1034=TV Code
1035=DFP code
1036=Mobile BIOS

;do not forgot to place spaces for this control
1037=   I&nitialization
1038= General Initialization STRAP Register
1039=AGP SBA Disabled
1039_h=NV_PEXTDEV_BOOT_0_STRAP_AGP_SBA_DISABLED
1040=FW Disabled (?)
1040_h=no hint
1041=STRAP Overwrite Enabled
1041_h=no hint
1042= Memory Clock tables
1043=GPU
1044=Memory
1045=Type
1046= TV Modes
1047=TV Mode Source
1048_h=Use override - Use Boot Time TV Mode override^mUse Straps (default NTSC M) - Skip Boot Time TV Mode override
1049=TV Mode
1050_h=Will work only if Use override enabled
1051=   &Fonts
1052= Fonts
1053=Save
1054=Replace
1055=Edit
1056=Select language
1057=Last Opened Files
1058=Read From Memory
1059=Read and Save To File

;
; Hex editor
;
;
1100=Save
1100_h=Save changes and exit
1101=Cancel
1101_h=Cancel all changes and exit
1102=Copy
1103=Paste
1104=Undo
1105=Set Font...
1106=Go to
1107=Find
1108=Find next
1109=Goto Special Location
1110=PCI Header
1111=NVIDIA Control Block
1112=TV Mode Block
1113=Signon Message
1114=VESA Vendor Name
1115=VESA Product Name
1116=VESA Product Revision
1117=General Init Table
1118=Init Script Table
1119=Fonts Address Table 

;this is status line text
1120=Pos^p:^p 
;Messages in HEX Editor
1121=Goto position...
1122=(prefix "0x" or "$" means hex)
1123=Invalid position
1124=Data not found.
1125=Find...
1126=Put "t.." for text, "T.." for case insensitive, other look for HEX
1127=Tools

;
; Help system
;

1=Help
230=How to flash BIOS
6=General Tab
7=Initialization
8=Fonts

;
;
; Messages
;

3000=Error loading BIOS Image!
;
; %d used for formatin messages do not remove it
;
3001=File size %d^mActual bios size : %d
3002=Bab PCI Header!
3003=Error
3004=Not X-BIOS!
3005=Bad control block structure!
3006=Old unsupported Control Block!
3007=Signon message. Max length %d chars
3008=No
3009=Yes
3010=Present
3011=X-BIOS Editor (%s)
3012=Used %d chars
3013=Bad SubVendor ID! Must be valid HEX Value
3014=Bad Sub Device ID! Must be valid HEX Value
3015=Bad version numver!
3016=Wrong file size for selected font
3017=Not implemented yet!
3018=Device
3019=SubVendor devices
3020=Time out!
3021=Error reading current BIOS!
3022=Ok
3023=Cancel
3024=Pleasde restart application to take effect!
3025=Select Language
3026=Select interface language
3027=HEX Editor
3028=Vendors list

; new in release 130

3029_h=Duplicate with selected
: new in RC 3 build 150
3030=AGP
3030_h=Show AGP low level information
3031=AGP low level information

;AGP show table
3032=Error getting information!
3033=Adapter Information
3034=Vendor ID
3035=Device ID
3036=Device Name
3037=Latency Timer
3038=AGP Revision
3039=IRQ
3040=Maximum command queue depth
3041=Sub Vendor Information
3042=Sub Vendor Name

;old non translated items
3043_h=Select SubDevice ID
3044_h=Select Vendor Name from list

; AGP Table
3046=Sub Device Name
3047=AGP Status
3048=AGP Rates Supported
3049=Current AGP Transfer Rate
3050=SBA Supported
3051=SBA Enabled
3052=FastWrites Supported
3053=FastWrites Enabled
3054=Over 4Gb transfer
3055=Error opening device control!
3056=AGP Disabled
