; 
; Croatian
; 
; This file provided only for translation
; English is build in language for editor
;
; Format:
; number=Text  control text i.e. labels, buttons
; number_h=Hint for control
; some controls have no hint message like label
; some controls have no Text message like Edit controls
; use ^m for carriage return
; use & for underline char
; use ^p for space
;
; Translation by Sasa Cikes (sasa.cikes@hi.hinet.hr)
;

[Translations]

;Main Window

1001=X-BIOS Editor 
1002=&Otvori
1002_h=Otvara datoteku s BIOS-om
1003=&Spremi
1003_h=Sprema BIOS u datoteku
1004=Hex editor
1004_h=Pokreće hex editor
1005=Opcije
1005_h=Opcije
1006=Pomoć
1006_h=Pomoć pri korištenju programa
1007=O programu
1007_h=Informacije o programu
1008=Izlaz
1008_h=Izlaz iz programa

;do not forgot to place spaces for this control

1009=Općenito
1010=PCI informacijski blok
1011=Informacije pri podizanju sustava
1012=&Device ID
1013=&Promijeni
1014=Sub Vendor
1015=Sub Device ID
1016=Preskoči detekciju DDC monitora
1017=Omogući poruku o količini memorije

; to put Carriage return use ^m

1017_h=Ako je uključeno:^mIspisuje količinu memorije^mpri podizanju sustava
1018=Omogući poruku pri podizanju sustava
1018_h=Ako je uključeno:^mIspisuje poruku pri podizanju sustava
1019=Inženjersko izdanje
1019_h=Ako je uključeno:^mIspisuje "Engineering Release" pri podizanju ^msustava (može se isključiti bez posljedica)
1020=Komprimiraj pri spremanju
1021=Poruka pri podizanju sustava
1022=Tekst poruke
1023=Boja poruke
1024_h=Boja poruke^m7 - bijela
1025=Broj okvira
1026_h=Pauzira određeni broj okvira^mpri podizanju sustava.^m1 sekunda = 70 okvira^mTvornička vrijednost: 280
1027=Tekst verzije BIOS-a
1028=Verzija BIOS-a
1029=OEM tekst
1030=VESA proizvođač
1031=VESA proizvod
1032=VESA revizija
1033=OEM revizija
1034=TV kod
1035=DFP kod
1036=Mobilni BIOS

;do not forgot to place spaces for this control

1037=I&nicijalizacija
1038=Inicijalizacijski STRAP registar
1039=AGP SBA isključeno
1039_h=Ako je isključeno:^mAGP Side Band Addressing je uključen
1040=FW isključeno ?
1040_h=Ovo je opcija koja se još uvijek testira
1041=Prepisivanje STRAP registra uključeno
1042=Tabela memorijskih taktova
1043=Čip
1044=Memorija
1045=Tip
1046=TV modovi
1047=Izvor TV modova
1048_h=Use override - Use Boot Time TV Mode override^mUse Straps (default NTSC M) - Skip Boot Time TV Mode override
1049=TV mod
1050_h=Will work only if Use override enabled
1051=&Fontovi
1052=Fontovi
1053=Spremi
1054=Zamijeni
1055=Promijeni
1056=Odabir jezika
1057=Zadnje otvarane datoteke
1058=Učitaj iz memorije
1059=Učitaj i spremi u datoteku

;
; Hex editor
;

1100=Spremi
1100_h=Spremi promjene i izađi
1101=Odustani
1101_h=Odustani od promjena i izađi
1102=Kopiraj
1103=Zalijepi
1104=Korak nazad
1105=Postavi font...
1106=Idi na
1107=Pronađi
1108=Pronađi slijedeći
1109=Idi na specijalnu lokaciju
1110=PCI zaglavlje
1111=NVIDIA kontrolni blok
1112=TV mod blok
1113=Poruka pri podizanju sustava
1114=VESA proizvođač
1115=VESA proizvod
1116=VESA revizija
1117=Glavna inicijalizacijska tabela
1118=Tabela inicijalizacijskih skripti
1119=Tabela adresa fontova

;this is status line text

1120=Pozicija^p:^p 

;Messages in HEX Editor

1121=Idi na poziciju...
1122=(prefiks "0x" ili "$" označava heksadecimalnu vrijednost)
1123=Neispravna pozicija
1124=Podaci nisu pronađeni
1125=Pronađi...
1126=Unesite "t.." za tekst, "T.." za osjetljivost na velika i mala slova, ostalo za heksadecimalne vrijednosti
1127=Alati

;
; Help system
;

1=Pomoć
230=Kako nadograditi BIOS
6=Općenito
7=Inicijalizacija
8=Fontovi

;
; Messages
;

3000=Greška pri čitanju BIOS-a!

;
; %d used for formatin messages do not remove it
;

3001=Veličina datoteke: %d^mVeličina BIOS-a: %d
3002=Neispravno PCI zaglavlje!
3003=Greška
3004=Nije X-BIOS!
3005=Neispravna struktura kontrolnog bloka!
3006=Stari, nepodržani kontrolni blok!
3007=Tekst poruke. Maksimalna dužina: %d slova
3008=Ne
3009=Da
3010=Prisutan
3011=X-BIOS Editor (%s)
3012=Iskorišteno %d slova
3013=Neispravan SubVendor ID. Mora biti heksadecimalna vrijednost.
3014=Neispravan Sub Device ID. Mora biti heksadecimalna vrijednost.
3015=Neispravna verzija!
3016=Kriva dužina datoteke za odabranu veličinu fonta!
3017=Nije još implementirano!
3018=Uređaj
3019=SubVendor uređaji
3020=Time Out!
3021=Greška pri čitanju trenutnog BIOS-a!
3022=U redu
3023=Odustani
3024=Promjene će nastupiti nakon ponovnog pokretanja programa!
3025=Odabir jezika
3026=Odaberite jezik sučelja
3027=Hex editor
3028=Lista proizvođača

; new in release 130

3029_h=Duplicate with selected
: new in RC 3 build 150
3030=AGP
3030_h=Show AGP low level information
3031=AGP low level information

;AGP show table
3032=Error getting information!
3033=Adapter Information
3034=Vendor ID
3035=Device ID
3036=Device Name
3037=Latency Timer
3038=AGP Revision
3039=IRQ
3040=Maximum command queue depth
3041=Sub Vendor Information
3042=Sub Vendor Name

;old non translated items
3043_h=Select SubDevice ID
3044_h=Select Vendor Name from list

; AGP Table
3046=Sub Device Name
3047=AGP Status
3048=AGP Rates Supported
3049=Current AGP Transfer Rate
3050=SBA Supported
3051=SBA Enabled
3052=FastWrites Supported
3053=FastWrites Enabled
3054=Over 4Gb transfer
3055=Error opening device control!
3056=AGP Disabled
